[valueport]
	databasekey = "SCOPE"
	view = packetdata
	datatype = "%24c"
	row = 3
	column = 1
	title = "SCOPE  date"
	displayrate = "F32ST28"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highcyan
	valuecolor = highcyan
	border = off
[valueport]
	databasekey = "Wave"
	view = packetdata
	byteindex = 54
	datatype = "%5hu"
	row = 3
	column = 60
	title = "Wave count"
	displayrate = "F32ST02"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highcyan
	valuecolor = highcyan
	border = off
[valueport]
	databasekey = "Trig"
	view = packetdata
	byteindex = 56
	rawformat = "%14.6e"
	displayformat = "%10.2e"
	row = 6
	column = 1
	title = "Trig level"
	units = "V"
	displayrate = "F32ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highgreen
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = 0.
[valueport]
	databasekey = "Trig"
	view = packetdata
	byteindex = 60
	rawformat = "%14.6e"
	displayformat = "%4.1f"
	row = 6
	column = 15
	title = "Trig delay"
	units = "%"
	displayrate = "F32ST05"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highgreen
	border = off
[valueport]
	databasekey = "Time"
	view = packetdata
	byteindex = 64
	rawformat = "%14.6e"
	displayformat = "%10.2e"
	row = 6
	column = 30
	title = "Time div"
	units = "s"
	displayrate = "F32ST07"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highgreen
	border = off
[valueport]
	databasekey = "Volts/div"
	view = packetdata
	byteindex = 68
	datatype = "%10.3e"
	row = 6
	column = 45
	title = "Volts/div 1"
	units = "V"
	displayrate = "F32ST04"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highgreen
	border = off
[valueport]
	databasekey = "Volts/div"
	view = packetdata
	byteindex = 72
	rawformat = "%14.6e"
	displayformat = "%10.2e"
	row = 6
	column = 60
	title = "Volts/div 2"
	units = "V"
	displayrate = "F32ST18"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highgreen
	border = off
[valueport]
	databasekey = "X"
	view = packetdata
	byteindex = 82
	rawformat = "%14.6e"
	displayformat = "%10.3e"
	row = 9
	column = 7
	title = "X chan 1"
	units = "s"
	displayrate = "F04ST04"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highred
	valuecolor = highred
	border = off
[valueport]
	databasekey = "Y"
	view = packetdata
	byteindex = 90
	rawformat = "%14.6e"
	displayformat = "%10.3e"
	row = 9
	column = 26
	title = "Y chan 1"
	units = "V"
	displayrate = "F04ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highred
	valuecolor = highred
	border = off
[valueport]
	databasekey = "X"
	view = packetdata
	byteindex = 86
	rawformat = "%14.6e"
	displayformat = "%10.3e"
	row = 9
	column = 46
	title = "X chan 2"
	units = "s"
	displayrate = "F04ST03"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highred
	valuecolor = highred
	border = off
[valueport]
	databasekey = "Y"
	view = packetdata
	byteindex = 94
	rawformat = "%14.6e"
	displayformat = "%10.3e"
	row = 9
	column = 65
	title = "Y chan 2"
	units = "V"
	displayrate = "F04ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highred
	valuecolor = highred
	border = off
[valueport]
	databasekey = "X"
	view = packetdata
	byteindex = 80
	datatype = "%5hu"
	row = 24
	column = 33
	units = "X"
	displayrate = "F01ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = yellow
	valuecolor = yellow
	border = off
[valueport]
	databasekey = "Y"
	view = packetdata
	byteindex = 76
	datatype = "%6hd"
	row = 13
	column = 1
	units = "Y"
	displayrate = "F01ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = yellow
	valuecolor = yellow
	border = off
	[plotport]
		row = 23
		column = 1
		width = 39
		height = 10
		title = "Channel 1"
		axiscolor = black
		axislabelcolor = black
		backgroundcolor = lightgrey
		bordercolor = white
		gridcolor = black
		plotcolor = yellow
		titlecolor = black
		xlower = 0.
		ylower = 0.
		xupper = 50000.
		yupper = 150.
		maxpoints = 1024
		plotgrid = on
[valueport]
	databasekey = "X"
	view = packetdata
	byteindex = 80
	datatype = "%5hu"
	row = 24
	column = 73
	units = "X"
	displayrate = "F01ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highmagenta
	valuecolor = highmagenta
	border = off
[valueport]
	databasekey = "Y"
	view = packetdata
	byteindex = 78
	datatype = "%6hd"
	row = 13
	column = 41
	units = "Y"
	displayrate = "F01ST01"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highmagenta
	valuecolor = highmagenta
	border = off
	[plotport]
		row = 23
		column = 41
		width = 39
		height = 10
		title = "Channel 2"
		axiscolor = highmagenta
		axislabelcolor = highmagenta
		backgroundcolor = blue
		bordercolor = white
		gridcolor = lightgrey
		plotcolor = highcyan
		titlecolor = highmagenta
		xlower = 0.
		ylower = 0.
		xupper = 50000.
		yupper = 150.
		maxpoints = 1024
		plotgrid = on
[valueport]
	databasekey = "Oscilloscope"
	view = page_no
	datatype = "%0c"
	row = 34
	column = 6
	title = "Oscilloscope TRACE "
	units = "50000 pt timebase    "
	displayrate = "F32ST04"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	drawenable = off
