[valueport]
	databasekey = "SENSORS"
	view = page_no
	datatype = "%0c"
	row = 34
	column = 6
	title = "SENSORS"
	units = "                     "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	drawenable = off
[valueport]
	databasekey = "Mag1"
	view = packetheader
	byteindex = 90
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 6
	column = 1
	title = "  Mag1 x   "
	units = " "
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highred
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Mag1"
	view = packetheader
	byteindex = 92
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 6
	column = 16
	title = "  Mag1 y   "
	units = " "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Mag1"
	view = packetheader
	byteindex = 94
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 6
	column = 31
	title = "  Mag1 z   "
	units = " "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 40
	rawformat = "%5hu"
	displayformat = "%6.2f"
	row = 6
	column = 46
	title = " Azi Meas 1  "
	units = "deg"
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Mag1"
	view = packetheader
	byteindex = 114
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 62
	title = " Mag1 "
	units = " "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highcyan
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000002
[valueport]
	databasekey = "Mag2"
	view = packetheader
	byteindex = 114
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 71
	title = " Mag2 "
	units = " "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highmagenta
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000003
[valueport]
	databasekey = "Mag2"
	view = packetheader
	byteindex = 106
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 11
	column = 1
	title = "  Mag2 x   "
	units = " "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Mag2"
	view = packetheader
	byteindex = 108
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 11
	column = 16
	title = "  Mag2 y   "
	units = " "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highmagenta
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Mag2"
	view = packetheader
	byteindex = 110
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 11
	column = 31
	title = "  Mag2 z   "
	units = " "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 40
	rawformat = "%5hu"
	displayformat = "%6.2f"
	row = 11
	column = 46
	title = " Azi Meas 2  "
	units = "deg"
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 38
	rawformat = "%5hu"
	displayformat = "%6.2f"
	row = 11
	column = 63
	title = "   Azi Cal   "
	units = "deg "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Accel"
	view = packetheader
	byteindex = 100
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 16
	column = 1
	title = "  Accel A  "
	units = "  "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Accel"
	view = packetheader
	byteindex = 102
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 16
	column = 16
	title = "  Accel B  "
	units = "  "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Accel"
	view = packetheader
	byteindex = 104
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 16
	column = 31
	title = "  Accel C  "
	units = "  "
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highgreen
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 16
	column = 46
	title = "  Elev Meas  "
	units = "deg "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 16
	column = 63
	title = "  Elev  Cal  "
	units = "deg  "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Gyro"
	view = packetheader
	byteindex = 96
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 21
	column = 1
	title = "  Gyro Fine "
	units = "   "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Gyro"
	view = packetheader
	byteindex = 98
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 21
	column = 16
	title = " Gyro Coarse"
	units = "   "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Gyro"
	view = packetheader
	byteindex = 112
	rawformat = "%hd"
	displayformat = "%5.0f"
	row = 21
	column = 31
	title = "  Gyro 2   "
	units = " "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -2048.
[valueport]
	databasekey = "Shaft"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 21
	column = 46
	title = "  Shaft Enc  "
	units = "deg  "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highcyan
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Gyro1"
	view = packetheader
	byteindex = 114
	rawformat = "%hu"
	displayformat = "%3c"
	row = 21
	column = 62
	title = " Gyro1 "
	units = " "
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highred
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000004
[valueport]
	databasekey = "Gyro2"
	view = packetheader
	byteindex = 114
	rawformat = "%hu"
	displayformat = "%3c"
	row = 21
	column = 71
	title = " Gyro2 "
	units = " "
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = highgreen
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000005
[valueport]
	databasekey = "Manual"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 1
	title = " Manual "
	units = " "
	displayrate = "F08ST04"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000006
[valueport]
	databasekey = "Auto"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 16
	title = " Auto "
	units = " "
	displayrate = "F08ST07"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000006
[valueport]
	databasekey = "Slew"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 29
	title = " Slew "
	units = " "
	displayrate = "F08ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000005
[valueport]
	databasekey = "Coarse"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 41
	title = " Coarse "
	units = " "
	displayrate = "F08ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000004
[valueport]
	databasekey = "Fine"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 54
	title = " Fine "
	units = " "
	displayrate = "F08ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000004
[valueport]
	databasekey = "Tracking"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 26
	column = 67
	title = "Tracking"
	units = "  "
	displayrate = "F08ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000001
