[valueport]
	databasekey = "Plot"
	view = page_no
	datatype = "%0c"
	row = 34
	column = 6
	title = "Plot demonstration"
	units = "                     "
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	drawenable = off
[valueport]
	databasekey = "secs"
	view = packetheader
	byteindex = 18
	rawformat = "%lu"
	displayformat = "%7.0f"
	row = 31
	column = 29
	units = "secs"
	displayrate = "F01ST01"
	backgroundcolor = lightgrey
	bordercolor = white
	titlecolor = magenta
	valuecolor = red
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -693792000.
[valueport]
	databasekey = "Azi."
	view = packetheader
	byteindex = 82
	rawformat = "%hd"
	displayformat = "%4.2f"
	row = 5
	column = 2
	title = "Azi. Error"
	units = "degs"
	displayrate = "F01ST01"
	backgroundcolor = lightgrey
	bordercolor = white
	titlecolor = magenta
	valuecolor = red
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
	[plotport]
		row = 30
		column = 1
		width = 40
		height = 25
		xtitle = "Time (seconds)"
		ytitle = "Azi Err"
		title = "Azimuth Error"
		axiscolor = magenta
		axislabelcolor = magenta
		backgroundcolor = lightgrey
		bordercolor = white
		gridcolor = white
		plotcolor = black
		titlecolor = magenta
		xlower = 0.
		ylower = -1.
		xupper = 200.
		yupper = 1.
		lineplot = on
		plotgrid = on
		forwardplot = on
[valueport]
	databasekey = "secs"
	view = packetheader
	byteindex = 18
	rawformat = "%lu"
	displayformat = "%7.0f"
	row = 17
	column = 66
	units = "secs"
	displayrate = "F01ST01"
	backgroundcolor = cyan
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -693792000.
[valueport]
	databasekey = "Elevation"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%5.1f"
	row = 5
	column = 42
	title = "Elevation"
	units = "degs"
	displayrate = "F01ST01"
	backgroundcolor = cyan
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
	[plotport]
		row = 16
		column = 42
		width = 36
		height = 11
		xtitle = "Time (s)"
		ytitle = "Elev"
		title = "Elev. Target Acq."
		axiscolor = cyan
		axislabelcolor = cyan
		backgroundcolor = cyan
		bordercolor = white
		gridcolor = black
		plotcolor = highcyan
		titlecolor = yellow
		xlower = 0.
		ylower = -44.
		xupper = 200.
		yupper = -39.
		lineplot = on
		plotgrid = on
		forwardplot = on
[valueport]
	databasekey = "secs"
	view = packetheader
	byteindex = 18
	rawformat = "%lu"
	displayformat = "%7.0f"
	row = 31
	column = 66
	units = "secs"
	displayrate = "F01ST01"
	backgroundcolor = cyan
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.
			a0 = -693792000.
[valueport]
	databasekey = "Azimuth"
	view = packetheader
	byteindex = 40
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 19
	column = 42
	title = "Azimuth"
	units = "degs"
	displayrate = "F01ST01"
	backgroundcolor = cyan
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -100.
	[plotport]
		row = 29
		column = 42
		width = 36
		height = 10
		xtitle = "Time (s)"
		ytitle = "Azi"
		title = "Azi - 100 degs"
		axiscolor = cyan
		axislabelcolor = cyan
		backgroundcolor = cyan
		bordercolor = white
		gridcolor = black
		plotcolor = highcyan
		titlecolor = yellow
		xlower = 0.
		ylower = -4.
		xupper = 200.
		yupper = 1.
		lineplot = on
		plotgrid = on
		forwardplot = on
