[valueport]
	databasekey = "Tuning/Performance"
	view = tps_secs
	datatype = "%0c"
	row = 34
	column = 6
	title = "Tuning/Performance"
	units = "                     "
	displayrate = "F01ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = red
	border = off
	drawenable = off
[valueport]
	databasekey = "Packets"
	view = vtelfr_cnt
	rawformat = "%11ld"
	displayformat = "%10lu"
	row = 9
	column = 2
	mnemonic = "Packets Received"
	units = "(PKTSRD)"
	displayrate = "F32ST18"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
[valueport]
	databasekey = "Tuning"
	view = tps_secs
	datatype = "%0c"
	row = 5
	column = 20
	mnemonic = "Tuning and Performance Samples Page 24"
	displayrate = "F01ST01"
	backgroundcolor = magenta
	bordercolor = white
	titlecolor = yellow
	valuecolor = red
	drawenable = off
[valueport]
	databasekey = "Measured"
	view = meanallfr_usecs
	rawformat = "%11ld"
	displayformat = "%8.3f"
	row = 21
	column = 41
	mnemonic = "Measured Rate"
	units = "Pkts/sec"
	displayrate = "F32ST20"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			function = reciprocal
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1000000.
			a0 = 0.
[valueport]
	databasekey = "Measured_Bit_Rate"
	view = tps_stats
	byteindex = 52
	rawformat = "%11ld"
	displayformat = "%10lu"
	row = 12
	column = 2
	mnemonic = "Measured_Bit_Rate"
	units = "(BITRTRI)"
	displayrate = "F32ST14"
	backgroundcolor = white
	bordercolor = black
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0
			a3 = 0
			a2 = 0
			a1 = 8
			a0 = 0
[valueport]
	databasekey = "Percentage_Buffer_Fu"
	view = tps_stats
	byteindex = 216
	rawformat = "%11ld"
	displayformat = "%7.2lf"
	row = 18
	column = 2
	mnemonic = "Percentage_Buffer_Full"
	units = "(RDPERC)"
	displayrate = "F32ST09"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 9.765625e-002
			a0 = 0.
[valueport]
	databasekey = "Measured_Pkt_Rate"
	view = tps_stats
	byteindex = 68
	datatype = "%8lu"
	row = 15
	column = 2
	mnemonic = "Measured_Pkt_Rate"
	units = "(PKTRTRDA)"
	displayrate = "F32ST04"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			quotient = 10
			a4 = 0
			a3 = 0
			a2 = 0
			a1 = 1
			a0 = 0
[valueport]
	databasekey = "Demanded_Loop_Time"
	view = tps_loop_time
	rawformat = "%11ld"
	displayformat = "%7lu"
	row = 24
	column = 2
	mnemonic = "Demanded_Loop_Time"
	units = "Loop-time"
	displayrate = "F32ST28"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
[valueport]
	databasekey = "Measured_Loop_Time"
	view = meanallfr_usecs
	rawformat = "%11ld"
	displayformat = "%7.0f"
	row = 24
	column = 41
	mnemonic = "Measured_Loop_Time"
	units = "Loop-meas"
	displayrate = "F32ST12"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-003
			a0 = 0.
[valueport]
	databasekey = "Over-clocking"
	view = tps_flags
	rawformat = "%8lx"
	displayformat = "%3c"
	row = 9
	column = 43
	mnemonic = "Over-clocking"
	displayrate = "F32ST07"
	backgroundcolor = lightgrey
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00008000
[valueport]
	databasekey = "Demanded_Rate"
	view = tps_loop_time
	rawformat = "%11ld"
	displayformat = "%8.3f"
	row = 21
	column = 2
	mnemonic = "Demanded_Rate"
	units = "Pkts/sec"
	displayrate = "F32ST32"
	backgroundcolor = white
	bordercolor = blue
	titlecolor = black
	valuecolor = magenta
	[calibration]
		function = polynomial
		[polynomial]
			function = reciprocal
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1000.
			a0 = 0.
