[valueport]
	databasekey = "CONTROL"
	view = page_no
	datatype = "%0c"
	row = 34
	column = 6
	title = "       CONTROL       "
	units = "                     "
	displayrate = "F32ST14"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	border = off
	drawenable = off
[valueport]
	databasekey = "Manual"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 1
	title = " Manual "
	units = " "
	displayrate = "F08ST02"
	backgroundcolor = black
	bordercolor = white
	titlecolor = highgreen
	valuecolor = highred
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000006
[valueport]
	databasekey = "Auto"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 16
	title = " Auto "
	units = " "
	displayrate = "F08ST04"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000006
[valueport]
	databasekey = "Slew"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 29
	title = " Slew "
	units = " "
	displayrate = "F08ST07"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000005
[valueport]
	databasekey = "Coarse"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 41
	title = " Coarse "
	units = " "
	displayrate = "F08ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = nonoffbit
		[bitoperation]
			bitmask = 0x00000004
[valueport]
	databasekey = "Fine"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 54
	title = " Fine "
	units = " "
	displayrate = "F08ST05"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000004
[valueport]
	databasekey = "Tracking"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 6
	column = 67
	title = "Tracking"
	units = "  "
	displayrate = "F08ST07"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000001
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 60
	rawformat = "%hu"
	displayformat = "%3c"
	row = 11
	column = 1
	title = "Elev Ctrl"
	units = "  "
	displayrate = "F08ST07"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000007
[valueport]
	databasekey = "Rack"
	view = packetheader
	byteindex = 70
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 11
	column = 15
	title = "Rack Temp "
	units = "deg C"
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 0.2443
			a0 = -773.
[valueport]
	databasekey = "Az"
	view = packetheader
	byteindex = 72
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 11
	column = 32
	title = "Az Motor Temp "
	units = "deg C"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 0.2443
			a0 = -773.
[valueport]
	databasekey = "El"
	view = packetheader
	byteindex = 74
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 11
	column = 49
	title = "El Motor Temp "
	units = "deg C"
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 0.2443
			a0 = -773.
[valueport]
	databasekey = "Motor"
	view = packetheader
	byteindex = 114
	rawformat = "%hu"
	displayformat = "%3c"
	row = 11
	column = 67
	title = "Motor Pwr"
	units = "  "
	displayrate = "F08ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = onoffbit
		[bitoperation]
			bitmask = 0x00000001
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 30
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 16
	column = 1
	title = "  Azi Dem   "
	units = "deg"
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 38
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 16
	column = 17
	title = "  Azi Cal  "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 32
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 16
	column = 33
	title = "  Elev Dem  "
	units = "deg"
	displayrate = "F04ST02"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Latitude"
	view = packetheader
	byteindex = 44
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 16
	column = 49
	title = "  Latitude  "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Longitude"
	view = packetheader
	byteindex = 46
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 16
	column = 65
	title = " Longitude  "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Azi"
	view = packetheader
	byteindex = 40
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 21
	column = 1
	title = "  Azi Meas  "
	units = "deg"
	displayrate = "F04ST03"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 21
	column = 17
	title = "  Elev Cal "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "Elev"
	view = packetheader
	byteindex = 42
	rawformat = "%hd"
	displayformat = "%5.2f"
	row = 21
	column = 33
	title = "  Elev Meas "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
[valueport]
	databasekey = "R.A"
	view = packetheader
	byteindex = 48
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 21
	column = 49
	title = "    R.A     "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = 0.
[valueport]
	databasekey = "Dec"
	view = packetheader
	byteindex = 50
	rawformat = "%hd"
	displayformat = "%6.2f"
	row = 21
	column = 65
	title = "    Dec     "
	units = "deg"
	displayrate = "F04ST01"
	backgroundcolor = blue
	bordercolor = white
	titlecolor = white
	valuecolor = yellow
	[calibration]
		function = polynomial
		[polynomial]
			a4 = 0.
			a3 = 0.
			a2 = 0.
			a1 = 1.e-002
			a0 = -90.
